Part I:

Resetn is a synchronous active low signal. To reset the FSM, force resetn to be 0.